Router TP-LINK TL-WR841N

Manuales: Ficha técnica, Guía rápida, Manual de usuario.

Software del fabricante: Asistente de configuración, Firmware 150320

Software de terceros: DD-WRT, OpenWrt / Openwrt.org, OpenWrt firmware para WR841N v9

Hardware v9

The port indexes in OpenWRT and in hardware (on the case) are swapped:

Port	index in /etc/config/network
CPU	0
1	4
2	3
3	2
4	1

It is possible to run 802.1Q tags on these ports. As of Chaos Calmer mixed (tagged/untagged) VLANs are working, and can be configured via LUCI. The maximum VLAN number is 15.

eth1 is directly connected to the WAN port.